Developed by ZeroDocs.com

SECTION 01 56 26 – TEMPORARY FENCING

1. GENERAL
	1. ADMINISTRATIVE REQUIREMENTS
		1. Pre-Installation Conference:
			1. Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder] and fence installer.
			2. Review: Project conditions, proposed fencing locations, and installation schedule.
	2. SUBMITTALS
		1. Action Submittals:
			1. Product Data: Manufacturer’s descriptive data and product attributes.
			2. Samples: Verification samples.
2. PRODUCTS
	1. MANUFACTURERS
		1. Contract Documents are based on products by Scepter, [www.scepterposts.com](http://www.scepterposts.com).
		2. Substitutions: [Refer to Division 01.] [Not permitted.]
	2. COMPONENTS
		1. Fence Posts:
			1. Product: Scepter Post, Multi-Fence Heavy Duty.
			2. Length: 60 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Posts:
			1. Product: Scepter Post, Standard Heavy Duty.
			2. Length: 60 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Posts:
			1. Product: Scepter Post, Multi-Fence Lite.
			2. Length: 60 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Posts:
			1. Product: Scepter Post, Standard Lite.
			2. Length: 60 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Posts:
			1. Product: Scepter Post, Silt Pole HD.
			2. Length: 39.4 inches.
		2. Fence Mesh:
			1. Product: Barrier Fence.
			2. Height: 48 inches.
			3. Opening size: 1.5 x 1.5 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Mesh:
			1. Product: Barricade Fence.
			2. Height: 48 inches.
			3. Opening size: 1.5 x 2.5 inches.
			4. Thickness: 0.0125 inch.

 \*\*\*\* OR \*\*\*\*

* + 1. Fence Mesh:
			1. Product: Snow Control Fence.
			2. Height: 48 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Mesh:
			1. Product: Snow Fence.
			2. Height: 48 inches.
			3. Opening size: 1.25 x 2 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Mesh:
			1. Product: Yard Fence.
			2. Height:48 inches.
			3. Opening size: 1.5 x 1.5 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Fabric:
			1. Product: Silt Fence.
			2. Height: 36 inches.
			3. Sieve size: No. 30 (0.023 inch).
		2. Caution Tape:
			1. Product: Caution Tape.
			2. Height: \_\_\_\_ inches.
			3. Color: [Red.] [Yellow.]
			4. Lettering: [CAUTION.] [DANGER.] [DO NOT ENTER.]
1. EXECUTION
	1. INSTALLATION
		1. Install in accordance with manufacturer’s instructions.
		2. Maximum fence post spacing: [\_\_] feet on center.

END OF SECTION