
Developed by ZeroDocs.com

SECTION 01 56 26 – TEMPORARY FENCING

1. GENERAL
   1. ADMINISTRATIVE REQUIREMENTS
      1. Pre-Installation Conference:
         1. Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder] and fence installer.
         2. Review: Project conditions, proposed fencing locations, and installation schedule.
   2. SUBMITTALS
      1. Action Submittals:
         1. Product Data: Manufacturer’s descriptive data and product attributes.
         2. Samples: Verification samples.
2. PRODUCTS
   1. MANUFACTURERS
      1. Contract Documents are based on products by Scepter, [www.scepterposts.com](http://www.scepterposts.com).
      2. Substitutions: [Refer to Division 01.] [Not permitted.]
   2. COMPONENTS
      1. Fence Posts:
         1. Product: Scepter Post, Multi-Fence Heavy Duty.
         2. Length: 60 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Posts:
       1. Product: Scepter Post, Standard Heavy Duty.
       2. Length: 60 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Posts:
       1. Product: Scepter Post, Multi-Fence Lite.
       2. Length: 60 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Posts:
       1. Product: Scepter Post, Standard Lite.
       2. Length: 60 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Posts:
       1. Product: Scepter Post, Silt Pole HD.
       2. Length: 39.4 inches.
    2. Fence Mesh:
       1. Product: Barrier Fence.
       2. Height: 48 inches.
       3. Opening size: 1.5 x 1.5 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Mesh:
       1. Product: Barricade Fence.
       2. Height: 48 inches.
       3. Opening size: 1.5 x 2.5 inches.
       4. Thickness: 0.0125 inch.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Mesh:
       1. Product: Snow Control Fence.
       2. Height: 48 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Mesh:
       1. Product: Snow Fence.
       2. Height: 48 inches.
       3. Opening size: 1.25 x 2 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Mesh:
       1. Product: Yard Fence.
       2. Height:48 inches.
       3. Opening size: 1.5 x 1.5 inches.

\*\*\*\* OR \*\*\*\*

* + 1. Fence Fabric:
       1. Product: Silt Fence.
       2. Height: 36 inches.
       3. Sieve size: No. 30 (0.023 inch).
    2. Caution Tape:
       1. Product: Caution Tape.
       2. Height: \_\_\_\_ inches.
       3. Color: [Red.] [Yellow.]
       4. Lettering: [CAUTION.] [DANGER.] [DO NOT ENTER.]

1. EXECUTION
   1. INSTALLATION
      1. Install in accordance with manufacturer’s instructions.
      2. Maximum fence post spacing: [\_\_] feet on center.

END OF SECTION